Eurofox REFERENCE INFORMATION

For detailed instructions on how to fly this aircraft, see the Aircraft Handbook. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel
          450 Kgs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel.


VNE - Never Exceed Speed
          185 KM/H

VNO - Maximum Structural-Cruising Speed
          160 KM/H

VA - Maneuvering Speed
          140 KM/H

VFE - Maximum Flaps-Extended Speed
          110 KM/H

VS0 - Minimum steady flight speed (flaps up)
       Double    75 KM/H
       Solo      70 KM/H

VS1 - Minimum steady flight speed (flaps full)
       Double    65 KM/H
       Solo      60 KM/H


EGT  - Max   880 degr C

CHT  - Max   150 degr C

OILT - Min    50 degr C
       Max   140 degr C

OILP - Min   15 bar*0,1   
     - Max   50 bar*0,1

RPM  - Max  5800 (max 5 min )
     - Cont 5500
