Eurofox PROCEDURES 

For detailed instructions on how to fly this aircraft, see the Aircraft Handbook. For suggested speeds, see the Reference tab.

____________________________________
BEFORE STARTING ENGINE

[ ] Brakes -- TEST AND SET
[ ] Electrical Equipment -- OFF
[ ] Avionics Master Switch -- OFF

____________________________________
ENGINE START

[ ] Throttle -- OPEN 1/4 INCH
[ ] Propeller Area -- CLEAR
[ ] Master Switch -- ON
[ ] Magneto Switches L+R -- ON
[ ] Ignition Switch -- START (release when engine starts)

Then:

[ ] Oil Pressure -- CHECK
[ ] Avionics Master Switch -- ON

____________________________________
BEFORE TAKEOFF

[ ] Flight Instruments -- CHECK and SET
[ ] Seatbelts -- FASTENED
[ ] Doors -- Closed
[ ] Safetyparachute -- UNLOCKED
[ ] Fuel Selector Valve -- BOTH
[ ] Fuel Quantity -- CHECK
[ ] Fuel Checklight -- CHECK
[ ] Altimeter -- SET
[ ] Flight Controls -- FREE AND CORRECT
[ ] Elevator Trim -- SET for takeoff
[ ] Wing Flaps -- SET for takeoff (Half)
[ ] Throttle -- 3500 RPM
[ ] Magnetos -- CHECK L+R
    <150 RPM drop on each; <50 RPM drop between
[ ] Engine Instruments -- CHECK
[ ] Throttle -- 1500 RPM or less
[ ] Strobe Light -- AS DESIRED
[ ] Landing Light -- AS DESIRED
[ ] Radios -- SET
[ ] Brakes -- RELEASE

____________________________________
TAKEOFF

[ ] Throttle  -- FULL OPEN
[ ] Elevator Control -- LIFT NOSE WHEEL (at 70 Km/H)
[ ] Climb Speed --  110 Km/H

____________________________________
EN ROUTE CLIMB

[ ] Airspeed -- 120 Km/H
[ ] Throttle -- 90 %

____________________________________
CRUISE

[ ] Power -- 4000-4800 RPM
[ ] Elevator Trim -- ADJUST

____________________________________
DESCENT

[ ] Power -- AS DESIRED

____________________________________
BEFORE LANDING

[ ] Landing Lights -- ON

____________________________________
LANDING

[ ] Airspeed -- 110 Km/H 
[ ] Wing Flaps -- AS DESIRED
    Half < 110 Km/H
    Full < 100 Km/H
[ ] Touchdown -- MAIN WHEELS FIRST
[ ] Landing Roll -- LOWER NOSE WHEEL GENTLY
[ ] Braking -- MINIMUM REQUIRED

____________________________________
AFTER LANDING

[ ] Wing Flaps -- UP

____________________________________
SECURING AIRPLANE

[ ] Avionics Master Switch, Electrical Equipment -- OFF
[ ] Magneto Switches (L+R) -- OFF
[ ] Master Switch -- OFF


